{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["内部招标实施情况汇总表","议标实施情况汇总表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"内部招标实施情况汇总表","index":0,"n_rows":3,"n_cols":16,"rows_kept":3,"merged":[[0,0,0,15]],"flags":["formulas_cached_only"]}
["2025年1月项目内部招标实施情况汇总表"]
["序号","项目建设管理单位","项目序号","项目名称","项目内容","项目类型（工程施工、工程服务）","审批时间","开标时间","合同签订时间","估算、概算或预算（元）","招标金额（元）","中标单位","中标金额（元）","中标单位资质","下浮率","备注"]
[null,"本月无内部招标项目"]

{"sheet":"议标实施情况汇总表","index":1,"n_rows":10,"n_cols":15,"rows_kept":10,"merged":[[0,0,0,14],[2,0,3,0],[2,1,3,1],[4,0,5,0],[4,1,5,1],[6,0,9,0],[6,1,9,1]],"flags":["formulas_cached_only"]}
["2025年1月项目议标实施情况汇总表"]
["序号","项目建设管理单位","项目序号","项目名称","项目内容","项目类型（工程施工、工程服务）","审批时间","合同签订时间","集团批复金额（万元）","估算、概算或预算（元）","议标单位","议标合同金额（元）","议标单位资质","议标下浮率","备注"]
[1,"供水公司",1,"幸福北沙头围De63PE管改造工程","管道改造","工程施工","2024-12-23","2025-01-08",{"v":143500,"d":"143,500.00"},{"v":143540.56,"d":"143,540.56"},"珠海宏达建筑工程有限公司",{"v":129756.5,"d":"129,756.50"},"市政公用工程施工总承包叁级",{"v":0.1,"d":"10.00%"},"暂列金额5700.00元"]
[null,null,2,"昭信村村民住宅楼给水设施改造","管道改造","工程施工","2024-12-30","2025-01-10",{"v":270000,"d":"270,000.00"},{"v":262846.4,"d":"262,846.40"},"珠海市供水机械工程有限公司",{"v":249704.08,"d":"249,704.08"},"市政公用工程施工总承包贰级",{"v":0.05,"d":"5.00%"}]
[2,"海宜公司",1,"珠海市金湾区三灶镇三灶水质净化厂1.6MW分布式光伏项目监理服务","珠海市金湾区三灶镇三灶水质净化厂1.6MW分布式光伏项目监理服务","工程服务","2024-11-30","2025-01-02","/",{"v":130700,"d":"130,700.00"},"珠海经济特区建设监理有限公司",{"v":88888.88,"d":"88,888.88"},"电力工程监理甲级",{"v":0.31990145371078804,"d":"31.99%"}]
[null,null,2,"洁源餐厨厂厌氧攤顶部呼吸口加装臭气收集管道项目施工","在厌氧罐顶部呼吸口加装风机和臭气收集管道统一收集后输送到除臭系统进行集中处理","工程施工","2024-12-26","2024-12-31","/",{"v":119383.96,"d":"119,383.96"},"广东环森环保工程有限公司",{"v":98508.82,"d":"98,508.82"},"环保工程专业承包贰级",{"v":0.18360001551464694,"d":"18.36%"},"暂列金额5684.95元"]
[3,"西江建管公司",1,"西区水厂扩建工程水土保持验收","本项目工作内容包括但不限于以下:(1)完成建设项目水土保持验收相关工作,确保建设项目水土保持验收符合行政主管部门的要求。(2)编制水土保持验收报告及验收鉴定书，编制报告质量要求为:应符合我国的相关法规标准，顺利通过专家评审符合行政主管部门水土保持验收备案的要求。((3))组织召开水土保持验收专家评审会。(4)提供的报备验收材料通过政府相关部门备案审批，获得备案文件。","工程服务","2024-11-26","2025-01-07","/",{"v":37900,"d":"37,900.00"},"广东诚信达勘测咨询有限公司",{"v":10450,"d":"10,450.00"},"/",{"v":0.7242744063324538,"d":"72.43%"}]
[null,null,2,"三灶水质净化厂提标改造及扩建工程水土保持验收","本项目工作内容包括但不限于以下:(1)完成建设项目水土保持验收相关工作,确保建设项目水土保持验收符合行政主管部门的要求。(2)编制水土保持验收报告及验收鉴定书，编制报告质量要求为:应符合我国的相关法规标准，顺利通过专家评审符合行政主管部门水土保持验收备案的要求。((3))组织召开水土保持验收专家评审会。(4)提供的报备验收材料通过政府相关部门备案审批，获得备案文件。","工程服务","2024-11-27","2025-01-07","/",{"v":39200,"d":"39,200.00"},"广东诚信达勘测咨询有限公司",{"v":12000,"d":"12,000.00"},"/",{"v":0.6938775510204082,"d":"69.39%"}]
[null,null,3,"金岛路及金海岸大道供水管道改造工程一期工程施工图审查","负责本工程给排水等专业的施工图以及勘察报告的审查任务并出具施工图审查合格证。","工程服务","2025-01-03","2025-01-16","/",{"v":114097.02,"d":"114,097.02"},"珠海泰安建设工程咨询有限公司",{"v":91277.6,"d":"91,277.60"},"审查资质等级：市政一类",{"v":0.20000014023153279,"d":"20.00%"}]
[null,null,4,"唐家水厂二期工程白蚁防治","本项目工作内容为进行唐家水厂二期工程白蚁防治。本项目白蚁预防工程是根据白蚁的生物学习性与建筑物的特点，使用长效防治白蚁药剂进行处理，制造不利于白蚁生存的生态环境而达到预防白蚁的目的。白蚁防治范围和内容包括但不限于以下:\n1、室内地坪药物处理;\n2、各楼层墙体药物处理;\n3、门洞、管道井、管道出入口药物处理;\n4、伸缩缝、沉降缝药物处理;\n5、建筑物外墙边四周防蚁线药物处理等。\n6、建筑物墙体两侧及室内地坪均需要设置屏障，预防\n面积按建筑物面积计算;其中所有建筑物白蚁预防屏障需首尾连接紧贴基础和墙体，并且包围所有进出管道。","工程服务","2025-01-05","2025-01-16","/",{"v":8395.6,"d":"8,395.60"},"珠海市齐民环治服务有限公司",{"v":8216.6,"d":"8,216.60"},"/",{"v":0.021320691790938096,"d":"2.13%"}]